****************************************************************************

     Readme.txt for Touch Panel Driver CD-ROM

     Copyright(C) 2002-2005 Fujitsu Component Ltd.  All rights reserved.

****************************************************************************

Index:

 1. Content of this CD-ROM

 2. Details of the driver model
  2-1 Serial interface driver
  2-2 PS2 interface driver
  2-3 USB interface driver

----------------------------------------------------------------------------

 1. Content of this CD-ROM

    Folder tree of this CD-ROM 

     DriverCD  ---  Serial  ---  Ser-0530  ---  V10L27
                |            |-  Ser-0505  ---  V13L00
                |            |-  Ser-0501  ---  V40L00
                |            |-  Ser-0531  ---  V10L16
                |            |-  Ser-0522  ---  V12L20
                |
                |-  Ps2  ------  PS2-0523  ---  V19L44
                |            |-  PS2-0524  ---  V19L44
                |            |-  PS2-0525  ---  V19L44
                |            |-  PS2-0534  ---  V10L11
                |            |-  PS2-0522  ---  V12L20
                |
                |-  Usb  ------  USB-0526  ---  V19L43
                             |-  USB-0527  ---  V19L43
                             |-  USB-0532  ---  V10L13
                             |-  USB-0535  ---  V10L10
                             |-  USB-0522  ---  V12L20

 
   The folders of "Serial", "Ps2", and "Usb" are containing driver sets for 
   each interface of the device. 
   For example, please choose "Serial" folder if you use the serial interface device. 
   The sub-folders in the interface folder are driver models. 
   The drivers are different in the Device specification and the operating system (OS).   


   Attention:The path based on the folder with each Readme.txt file is mentioned in 
             Readme.txt file of the folder of each model.
             So,In case of folder and file designation are done when it is installed,
             Substitute the path of this CD for the path name mentioned in that 
             Readme.txt file, and specify it. 


 2. Details of the each driver model

  2-1 Serial interface driver

     Ser-0530\V10L27
     (model number NS01B-0559-0530) 

        This driver is for the following devices and OS. 
          Device   : N010-0559-V021,V031,V022,V032 (7wire,4wire,Non-PnP,PnP)
          OS       : Windows95,Windows98,WindowsMe,WindowsNT4,Windows2000,Windowsxp

        Please install the driver according to the instruction of the installer 
        "RTPsetup.exe" which starts automatically when CD-ROM is inserted. 
        Or, Please execute "Setup.exe", and install the driver. 
        The driver checks OS, and installs the driver in your system. 
        Please read "Readme.txt" in this folder about details of the installation. 


     Ser-0505\V13L00\DOS
     (model number NS01B-0559-0505) 

        This driver is for the following devices and OS. 
          Device   : N010-0559-V021,V031,V022,V032 (7wire,4wire,Non-PnP,PnP)
          OS       : MS-DOS

        Please read "Readme.txt" in this folder about details of the installation. 


     Ser-0501\V40L00\Win31
     (model number NS01B-0559-0501) 

        This driver is for the following devices and OS. 
          Device   : N010-0559-V021,V031,V022,V032 (7wire,4wire,Non-PnP,PnP)
          OS       : Windows3.1

        Please read "Readme.txt" in this folder about details of the installation. 


     Ser-0531\V10L16\WinCE
     (model number NS01B-0559-0531) 

        This driver is for the following devices and OS. 
          Device   : N010-0559-V021,V031,V022,V032 (7wire,4wire,Non-PnP,PnP)
          OS       : Windows CE 3.0/.Net/.Net4.1/.Net4.2/.Net5.0(x86)

        This device works in the platform of x86. This driver does not work in other platforms. 
        Please read "Readme.txt" in this folder about details of the installation. 


     Ser-0522\V12L20\Linux
     (model number NS01B-0559-0526) 

       This driver is for the following devices and OS. 
         Device   : N010-0559-V021,-V022,-V031,-V032 
         LINUX Kernel Version  : 2.2.14, 2.4.2, 2.4.18, 2.4.19, 2.4.20, 2.4.22
         Xfree86 Version : 3.3.6, 4.0.3, 4.2.0, 4.3.0

       Please read "ReadmeE.txt" in this folder about details of the installation. 
       The Serial,PS2,USB driver of Linux uses the same file.


  2-2 PS2 interface driver

     PS2-0523\V19L44
     (model number NS01B-0559-0523) 

        This driver is for the following devices and OS. 
          Device   : N010-0559-V043 (4wire Non-EEPROM)
          OS       : Windows98,WindowsMe,WindowsNT4,Windows2000,Windowsxp

       Please connect the device, and install standard PS2 mouse driver of Windows. 
       Afterwards, Please install the driver according to the instruction of the 
       installer "RTPsetup.exe" which starts automatically when CD-ROM is inserted. 
       Or, Please execute "TPSetup.exe", and install the driver. 
       The driver checks OS, and installs the driver in your system. 


     PS2-0524\V19L44
     (model number NS01B-0559-0524) 


       This driver is for the following devices and OS. 
         Device   : N010-0559-V051 (7wire EEPROM)
         OS       : Windows98,WindowsMe,WindowsNT4,Windows2000,Windowsxp

       Please connect the device, and install standard PS2 mouse driver of Windows. 
       Afterwards, Please install the driver according to the instruction of the 
       installer "RTPsetup.exe" which starts automatically when CD-ROM is inserted. 
       Or, Please execute "TPSetup.exe", and install the driver. 
       The driver checks OS, and installs the driver in your system. 


     PS2-0525\V19L44
     (model number NS01B-0559-0525) 

       This driver is for the following devices and OS. 
         Device   : N010-0559-V051 (7wire Non-EEPROM)
         OS       : Windows98,WindowsMe,WindowsNT4,Windows2000,Windowsxp

       Please connect the device, and install standard PS2 mouse driver of Windows. 
       Afterwards, Please install the driver according to the instruction of the 
       installer "RTPsetup.exe" which starts automatically when CD-ROM is inserted. 
       Or, Please execute "TPSetup.exe", and install the driver. 
       The driver checks OS, and installs the driver in your system. 


     Note : Because there is no standard architecture of PS2 in mobile PC system, there may happen
          some problem to use our touch panel driver. We must solve problem case by case.
          Especially some note PC BIOS makes modification to command data from PS2 controller
          to peripheral device. Our touch panel system does not work correctly in this kind of PC.


     PS2-0534\V10L11\WinCE41,PS2-0534\V10L11\WinCE42,PS2-0534\V10L11\WinCE50
     (model number NS01B-0559-0534) 

        This driver is for the following devices and OS. 
          Device   : N010-0559-V043,V051
          OS       : Windows CE .Net4.1/.Net4.2/.Net5.0(x86)

        This device works in the platform of x86. This driver does not work in other platforms. 
        Please read "Readme.txt" in this folder about details of the installation. 


     PS2-0522\V12L20\Linux
     (model number NS01B-0559-0526) 

       This driver is for the following devices and OS. 
         Device   : N010-0559-V041,-V042,-V043,-V051 
         LINUX Kernel Version : 2.2.14, 2.4.2, 2.4.18, 2.4.19, 2.4.20, 2.4.22
         Xfree86 Version : 3.3.6, 4.0.3, 4.2.0, 4.3.0

       Please read "ReadmeE.txt" in this folder about details of the installation. 
       The Serial,PS2,USB driver of Linux uses the same file. 


  2-3 USB interface driver

     USB-0526\V19L43
     (model number NS01B-0559-0526) 

       This driver is for the following devices and OS. 
         Device   : NC41120-0004 (4wire,Single Mode)
         OS       : Windows98,WindowsMe,Windows2000,Windowsxp

       Please connect the device, and install standard HID mouse driver of Windows. 
       Afterwards, Please install the driver according to the instruction of the 
       installer "RTPsetup.exe" which starts automatically when CD-ROM is inserted. 
       Or, Please execute "TPSetup.exe", and install the driver. 
       The driver checks OS, and installs the driver in your system. 


     USB-0527\V19L43
     (model number NS01B-0559-0527) 

       This driver is for the following devices and OS. 
         Device   : NC41120-0015 (7wire,Single Mode)
         OS       : Windows98,WindowsMe,Windows2000,Windowsxp

       Please connect the device, and install standard HID mouse driver of Windows. 
       Afterwards, Please install the driver according to the instruction of the 
       installer "RTPsetup.exe" which starts automatically when CD-ROM is inserted. 
       Or, Please execute "TPSetup.exe", and install the driver. 
       The driver checks OS, and installs the driver in your system. 


     USB-0532\V10L13\WinCE
     (model number NS01B-0559-0532) 

        This driver is for the following devices and OS. 
          Device   : NC41120-0004,-0015 (4wire,7wire)
          OS       : WindowsCE.Net4.1/.Net4.2/.Net5.0(x86)

        This device works in the platform of x86. This driver does not work in other platforms. 
        Please read "ReadmeE.txt" in this folder about details of the installation. 


     USB-0535\V10L10
     (model number NS01B-0559-0535) 

       This driver is for the following devices and OS. 
         Device   : NC41120-0015 (7wire,Dual Mode)
         OS       : Windows2000,Windowsxp

       Please read "WINUSBreadme_E.txt" in this folder about details of the installation. 


     USB-0522\V12L20\Linux
     (model number NS01B-0559-0526) 

       This driver is for the following devices and OS. 
         Device   : A1NC41120-0004
         LINUX Kernel Version : 2.4.2, 2.4.18, 2.4.19, 2.4.20, 2.4.22
         Xfree86 Version : 4.0.3, 4.2.0, 4.3.0

       Please read "ReadmeE.txt" in this folder about details of the installation. 
       The Serial,PS2,USB driver of Linux uses the same file. 

 