CE7 USB driver release note
[2015-04-25]Version 3.2.7.2825 for Single touch device
[2015-04-24]Version 3.3.7.2824 for PCAP
Bug Fixed:
     1. Fixed bug for Draw test tool will report wrong up event.


[2014-10-20]Version 3.2.7.2220 for Single touch device
[2014-10-20]Version 3.2.7.2221 for PCAP
Bug Fixed:
     1. Fixed bug for second contact will lose data issue.
     2. Fixed bug for touch can not work on the some system after suspend resume.

[2014-09-26]Version 3.2.7.2126 for Single touch device
[2014-09-25]Version 3.2.7.2125 for PCAP
Bug Fixed:
     Fixed bug for if the DrupNum parameter is not 0 , touchp maybe will lose report leave up.

[2014-09-10]Version 3.3.7.2101 for Single Touch device/PCAP7200 series
Bug Fixed:
1.fixed PCAP7200 series Firmware update tool can not get correct information and erase failed issue.

[2014-08-15]Version 3.3.7.2015 for PCAP
[2014-08-18]Version 3.3.7.2018 for Single Touch device
Bug Fixed:
1.fixed the touchp driver must be loaded before USB host device driver issue.
   modify the check registry architecture let touchp driver not need be loaded before USB host device driver.

[2014-07-29]Version 3.3.7.1929
Bug Fixed:
1. driver will check registry value every 100ms. 
    If system is have base ,this process will effect system performance.
    So modify this vesrion driver do not read  registry every 100ms.
    But it will has a side effect. The Touchp driver must be loaded before USB host device driver.
    If the touchp driver be loaded after USB host device driver, the touch will not work.
New Feature:
1. Add FixedRotateInfo parameter for rotate point coordinates.

[2014-06-18]Version 3.3.7.1918
Bug Fixed:
1. Some thread priority is too high. It will effect system performance.
    This version set these thread priority to normal level.

[2014-06-18]Version 3.3.7.1816
Bug Fixed:
1. Fixed 9 point calibration is not save correct calibration data in to device or system.

[2014-05-09]Version 3.3.7.1709
New Feature:
1. Mondify eGalaxTouch utility. Check registry key "CalSource".
    If the CalSource is into 0 , the utility will disable all calibration UI.

[2014-02-20]Version 3.3.7.1420
Bug Fixed:
1. Fixed for put wrong driver files into CEPC folder.

[2013-05-22]Version 3.3.7.0522
Bug Fixed:
1. Fixed driver will report wrong touch status for multi-touch point.

[2013-04-30]Version 3.3.7.0429
New feature
1. Support PCAP79xx series product.

[2013-03-01]Version 3.3.7.0301
New feature
1.Add halfVGA function for split display.

[2012-12-05] Version 3.2.7.1205
Bug Fixed :
1. fix driver report wrong multi-touch contact ID to system.

[2012-11-23] Version 3.2.7.1123

New feature :
1. Add edge Compensation function

Bug fixed : 
1. The driver will often lose point data